Contact Name:
	Howard Frazier

Contact Email:
	hfrazier@broadcom.com

What type of assignment/registration are you requesting?

Assignment of the following additions to the IANAifMauTypeListBits textual convention,
immediately following b1000BasePX20U(53) -- 1000BASE-PX20U:

	b10GbaseT(xx) -- 10GBASE-T
	b10GbaseLRM(xx) -- 10GBASE-LRM
	b1000baseKX(xx) -- 1000BASE-KX
	b10GbaseKX4(xx) -- 10GBASE-KX4
	b10GbaseKR(xx) -- 10GBASE-KR
	b10G1GbasePRXD1(xx) -- 10/1GBASE-PRX-D1 
	b10G1GbasePRXD2(xx) -- 10/1GBASE-PRX-D2
	b10G1GbasePRXD3(xx) -- 10/1GBASE-PRX-D3
	b10G1GbasePRXU1(xx) -- 10/1GBASE-PRX-U1
	b10G1GbasePRXU2(xx) -- 10/1GBASE-PRX-U2
	b10G1GbasePRXU3(xx) -- 10/1GBASE-PRX-U3
	b10GbasePRD1(xx) -- 10GBASE-PR-D1
	b10GbasePRD2(xx) -- 10GBASE-PR-D2
	b10GbasePRD3(xx) -- 10GBASE-PR-D3
	b10GbasePRU1(xx) -- 10GBASE-PR-U1
	b10GbasePRU3(xx) -- 10GBASE-PR-U3

Assignment of the following additions to the IANAifMauAutoNegCapBits textual
convention, immediately following b1000baseTFD(15) -- 1000BASE-T full duplex mode:

	b10GbaseT(xx) -- 10GBASE-T
	b1000baseKX(xx) -- 1000BASE-KX
	b10GbaseKX4(xx) -- 10GBASE-KX4
	b10GbaseKR(xx) -- 10GBASE-KR

Assignment of the following additions to the dot3MauType object identities, 
immediately following dot3MauType1000BasePX20U OBJECT-IDENTITY … 
::= { dot3MauType 53 }:

     dot3MauType10GbaseT OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "Four-pair Category 6A or better, full duplex mode only"
       REFERENCE   "[IEEE802.3], Clause 55"
       ::= { dot3MauType xx }

     dot3MauType10GbaseLRM OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "R 220 m multimode fiber over 1310 nm optics"
       REFERENCE   "[IEEE802.3], Clause 68"
       ::= { dot3MauType xx }

     dot3MauType1000baseKX OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "X backplane, full duplex mode only"
       REFERENCE   "[IEEE802.3], Clause 70"
       ::= { dot3MauType xx }

     dot3MauType10GbaseKX4 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "4 lane X backplane, full duplex mode only"
       REFERENCE   "[IEEE802.3], Clause 71"
       ::= { dot3MauType xx }

     dot3MauType10GbaseKR OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "R backplane, full duplex mode only"
       REFERENCE   "[IEEE802.3], Clause 72"
       ::= { dot3MauType xx }

     dot3MauType10G1GbasePRXD1 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber asymmetric EPON OLT, low power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

     dot3MauType10G1GbasePRXD2 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber asymmetric EPON OLT, medium power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

     dot3MauType10G1GbasePRXD3 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber asymmetric EPON OLT, high power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

     dot3MauType10G1GbasePRXU1 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber asymmetric EPON ONU, low power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

     dot3MauType10G1GbasePRXU2 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber asymmetric EPON ONU, medium power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

     dot3MauType10G1GbasePRXU3 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber asymmetric EPON ONU, high power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

     dot3MauType10GbasePRD1 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber symmetric EPON OLT, low power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

     dot3MauType10GbasePRD2 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber symmetric EPON OLT, medium power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

     dot3MauType10GbasePRD3 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber symmetric EPON OLT, high power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

     dot3MauType10GbasePRU1 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber symmetric EPON ONU, low power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

     dot3MauType10GbasePRU3 OBJECT-IDENTITY
       STATUS      current
       DESCRIPTION "One single-mode fiber symmetric EPON ONU, high power budget"
       REFERENCE   "[IEEE802.3], Clause 75"
       ::= { dot3MauType xx }

Which registry are you requesting this assignment/registration be made in?

The assignment of the IANAifMauTypeListBits and IANAifMauAutoNegCapBits textual conventions as well as the dot3MauType object identities is contained in the IANA-MAU-MIB, which is currently published as IETF RFC 4836. The IEEE 802.3 Ethernet Working Group is currently working on a project, known as IEEE P802.3.1, that will update and republish the IETF RFCs that are relevant to the management of Ethernet interfaces, including the contents of RFC 4836.

If possible, please give a brief description of why you need this assignment/registration:

The new MAU types and the associated AutoNeg capability bits listed above were specified in recently approved amendments to IEEE Std 802.3, including IEEE Std 802.3an-2006, IEEE Std 802.3aq-2007, IEEE Std 802.3ap-2007, and IEEE Std 802.3av-2009. The description of the IANAifMauTypeListBits textual convention states that “…changes in this textual convention SHALL be synchronized with relevant changes in the dot3MauType OBJECT-IDENTITIES." The assignments will be reflected in Clause 14 of IEEE P802.3.1, 
“IEEE Draft Standard for Management Information Base (MIB) definitions for Ethernet.”

Additional Information. Please include a reference to the specification or RFC (if available) that defines this number or name space: 

IEEE Std 802.3-2008, subclauses 30.5.1.1.2 aMAUType and 30.6.1.1.5 aAutoNegLocalTechnologyAbility, as amended by IEEE Std 802.3av-2009.