The channels folder includes sub-folders for three different crosstalk conditions

8F ( 8 FEXT)

5F3N ( 5 FEXT+3 NEXT)

In each of these folders

There are 10 channels with channel loss varying from 10 db to 35 db @14GHZ

<base\_name>\_t.s4p - Through channel s param files

<base\_name>\_f?.s4p – corresponding FEXT files

<base\_name>\_n?.s4p – corresponding NEXT files.

Channel port \_0rder is {1 2 3 4}