{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Action Items","D 1.0 tasks"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Action Items","index":0,"n_rows":33,"n_cols":48,"rows_kept":33,"cut":false,"hidden":false,"merged":[[1,2,1,22],[1,23,1,47],[2,2,2,3],[2,4,2,5],[2,6,2,8],[2,9,2,10],[2,11,2,12],[2,13,2,14],[2,15,2,16],[2,17,2,19],[2,45,2,46],[2,20,2,21],[2,23,2,24],[2,25,2,26],[2,27,2,28],[2,29,2,30],[2,42,2,44],[2,31,2,33],[2,36,2,37],[2,34,2,35],[2,38,2,39],[2,40,2,41]]}
[null,"On Track"]
[null,"Started, risk of being late",2018,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2019]
[null,"late","Mar",null,"Apr",null,"May",null,null,"Jun",null,"Jul",null,"Aug",null,"Sep",null,"Oct",null,null,"Nov",null,"Dec","Jan",null,"Feb",null,"Mar",null,"Apr",null,"May",null,null,"Jun",null,"Jul",null,"Aug",null,"Sep",null,"Oct",null,null,"Nov",null,"Dec"]
[null,"due date","7,8",21,4,18,2,16,"24,25",13,27,"PL",25,8,22,5,"IN",3,17,31,"PL",28,12,9,"IN",6,20,6,"PL",3,17,1,15,"IN",12,26,10,"PL",7,21,4,"IN",2,16,30,"PL",27,11]
[null,"OEM Topology"]
[null,"Consolidated Topology"]
[null,"OEM Power Consumption Expectations"]
[null,"PoDL and Power Budget"]
[null,"Cabling System Model - IL & RL"]
[null,"Thomas Mueller"]
[null,"Eric DiBiaso"]
[null,"Signaling type and modulation (2.5 Gb/s & 10 Gb/s)"]
[null,"Sujan Pandey"]
[null,"Tom Souvignier"]
[null,"Peter Wu"]
[null,"Ramin Farjad"]
[null,"Tazhi Madgar"]
[null,"Conrad Zerna"]
[null,"EMC testing"]
[null,"PHY Vendor Needs"]
[null,"Test Data"]
[null,"Line Coding and FEC "]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Register Maps"]
[null,"EEE support"]
[null,"PICs"]

{"sheet":"D 1.0 tasks","index":1,"n_rows":59,"n_cols":3,"rows_kept":59,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["What's still missing.  Major items only.  Minor stuff and corrections not covered here."]
["Based on ",0.3]
["Date updated",{"$f":" LastSaveDate()","v":"2018-05-24T09:27:19"}]
[]
["Clause","Who to contribute text","Comments"]
[30,"Natalie","Management\nMost of this can be completed as information is provided in Clauses 149 & 150."]
[44,null,"Introduction to 10 Gb/s baseband network\nNeed to complete additions to add 10GBASE-T1."]
[45,"Natalie","Management Data Input/Output (MDIO) Interface\nCollected from information in Clauses 149 & 150.\nShould OAM be added?"]
[78,null,"Energy-Efficient Ethernet (EEE)\nSomeone needs to provide the timing information for the rows to be added."]
["98B.3",null,"Need to add bit definitions for 2.5GBASE-T1, 5GBASE-T1 and 10GBASE-T1. "]
["98.B.4","Natalie","Add 2.5GBASE-T1, 5GBASE-T1 and 10GBASE-T1 to Priority Resolution list from fastest to slowest."]
[104,null,"PoDL"]
[125,null,"Introduction to 2.5 Gb/s and 5 Gb/s networks\nNeed to modify to add references to 2.5GBASE-T1 and 5GBASE-T1"]
["149, 149.1, 149.2","Natalie","Fill in open spots based on remainder of content in Clause 149."]
["149.1.2.1",null,"Overview - Physical Coding Sublayer (PCS)"]
["149.1.2.2",null,"Overview - Physical Medium Attachment (PMA) sublayer"]
["149.1.2.3",null,"EEE capability"]
["149.1.2.4",null,"Link Synchronization"]
["149.1.3",null,"Signaling"]
["149.1.4","Natalie","Interfaces "]
["149.1.5","Natalie","Conventions - similar in all PHY Clauses"]
[149.19999999999999,null,"2.5GBASE-T1 service primitives and interfaces"]
[149.30000000000001,null,"2.5GBASE-T1 Physical Coding Sublayer (PCS) functions\nAdd OAM?"]
[149.4,null,"Physical Medium Attachment (PMA) Sublayer"]
[149.5,null,"PMA electrical specifications"]
[149.6,null,"Management interface"]
[149.69999999999999,null,"Link Segment"]
["149.7.x","Natalie","Differential characteritic impedance\nNeed to decide if we want to put a tolerance on 100 ohms, e.g. 3%.\nNominal impedance of 100 ohms for cabling.  NO TOLERANCE!"]
["149.7.x",null," Differential to common mode conversion/ common mode to differential mode conversion"]
["149.7.x",null,"Maximum link delay"]
["149.7.x",null,"Coupling parameters between link segments - alien xtalk"]
["149.7.x",null,"Coupling attenuation"]
["149.7.x",null,"Transfer Impedance "]
[149.80000000000001,null,"MDI specification"]
[149.9,"Natalie","Environmental specifications\nText approved at March 2018 Interim"]
["149.10",null,"Delay constraints"]
[149.11000000000001,"Curtis","PICS"]
["150, 150.1, 150.2","Natalie","Fill in open spots based on remainder of content in Clause 150."]
["150.1.3.1",null,"Overview - Physical Coding Sublayer (PCS)"]
["150.1.3.2",null,"Overview - Physical Medium Attachment (PMA) sublayer"]
["150.1.3.3",null,"EEE capability"]
["150.1.3.4",null,"Link Synchronization"]
["150.1.4",null,"Signaling"]
["150.1.5","Natalie","Interfaces to be inserted prior to current 149.1.4 Conventions in this clause and after Signaling."]
["150.1.6","Natalie","Conventions - similar in all PHY Clauses"]
[150.19999999999999,null,"5GBASE-T1 and 10GBASE-T1 service primitives and interfaces"]
[150.30000000000001,null,"5GBASE-T1 and 10GBASE-T1 Physical Coding Sublayer (PCS) functions\nAdd OAM?"]
[150.4,null,"Physical Medium Attachment (PMA) Sublayer"]
[150.5,null,"PMA electrical specifications"]
[150.6,null,"Management interface"]
[150.69999999999999,null,"Link Segment"]
["150.7.x","Natalie","Differential characteritic impedance\nNeed to decide if we want to put a tolerance on 100 ohms, e.g. 3%."]
["150.7.x",null,"Do we need Differential to common mode conversion?"]
["150.7.x",null,"Maximum link delay"]
["150.7.x",null,"Coupling parameters between link segments"]
[150.80000000000001,null,"MDI specification"]
[150.9,"Natalie","Environmental specifications\nText approved at March 2018 Interim"]
["150.10",null,"Delay constraints"]
[150.11000000000001,"Curtis","PICS"]